|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| Structure of VIN system   |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  | | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | | ☆ | L | 4 | H | X | T | E | J | P | ? | ? | ? | ? | ? | ? | ? | ? | ? | ☆ |   Assembly plant code：  6: Assembly plants 1  7: Assembly plants 2  Running number：000001-999999  Production year:  2019： K 2020：L  2021： M 2022：N  Transmission type：Belt drire: P  Check Number calculated automatically. Possible character including:  **0, 1, 2, 3, 4, 5, 6, 7, 8, 9, X**  Engine type:  4 stroke air cooling horizontal: E  Vehicle type: motorscooter: T  Engine displacement: 125CC: J  Design NO.: X  WMI： L4H |