|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| Structure of VIN system

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ☆ | L | 4 | H | X | T | E | J | P | ? | ? | ? | ? | ? | ? | ? | ? | ? | ☆ |

Assembly plant code： 6: Assembly plants 17: Assembly plants 2Running number：000001-999999Production year:2019： K 2020：L2021： M 2022：NTransmission type：Belt drire: PCheck Number calculated automatically. Possible character including:**0, 1, 2, 3, 4, 5, 6, 7, 8, 9, X**Engine type: 4 stroke air cooling horizontal: EVehicle type: motorscooter: TEngine displacement: 125CC: JDesign NO.: XWMI： L4H |