|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| Structure of VIN system   |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  | | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | | ☆ | L | 4 | H | B | P | V | N | L | ? | ? | ? | ? | ? | ? | ? | ? | ? | ☆ |   Engine displacement:  250CC: N  Engine type:  vertical, V cylinder air cooling: V  Vehicle type:  two motorcycle: P  Design NO.: B  WMI： L4H  Transmission type：  Chain drive: L  Assembly plant code：  6: Assembly plants 1  7: Assembly plants 2  Running number：000001-999999  Production year:  2019： K 2020：L  2021： M 2022：N  Check Number calculated automatically. Possible character including:  **0, 1, 2, 3, 4, 5, 6, 7, 8, 9, X** |