|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| Structure of VIN system

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ☆ | L | 4 | H | C | P | V | N | L | ? | ? | ? | ? | ? | ? | ? | ? | ? | ☆ |

Engine displacement:  250CC: NEngine type: vertical, V cylinder air cooling: VVehicle type:  two motorcycle: PDesign NO.: CWMI： L4HTransmission type： Chain drive: LAssembly plant code： 6: Assembly plants 17: Assembly plants 2Running number：000001-999999Production year:2019： K 2020：L2021： M 2022：NCheck Number calculated automatically. Possible character including:**0, 1, 2, 3, 4, 5, 6, 7, 8, 9, X** |