|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| Structure of VIN system   |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  | | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | | ☆ | L | 4 | H | J | T | E | J | P | ? | ? | ? | ? | ? | ? | ? | ? | ? | ☆ |   `  Assembly plant code：  Assembly plants 1: 6  Assembly plants 2: 7  Production year:  2020： L 2021：M  2022： N 2023：P  Check Number calculated automatically. Possible character including:  **0, 1, 2, 3, 4, 5, 6, 7, 8, 9, X**  Running number：000001-999999  Engine type:  4 stroke, air cooling, horizontal: E  Transmission type：Belt drire: P  Vehicle type: scooter: T  Engine displacement: 125CC: J  Design NO.: J  WMI： L4H |