|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| Structure of VIN system

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ☆ | L | 4 | H | K | T | E | J | P | ? | ? | ? | ? | ? | ? | ? | ? | ? | ☆ |

`Assembly plant code：  Assembly plants 1: 6 Assembly plants 2: 7Production year:2020： L 2021：M2022： N 2023：PCheck Number calculated automatically. Possible character including:**0, 1, 2, 3, 4, 5, 6, 7, 8, 9, X**Running number：000001-999999Engine type: 4 stroke, air cooling, horizontal: ETransmission type：Belt drire: PVehicle type: scooter: TEngine displacement: 125CC: JDesign NO.: KWMI： L4H |