|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| Structure of VIN system   |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  | | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | | 🟊 | L | 4 | H | J | T | E | J | P | ? | H | 6 | 0 | 0 | 0 | 0 | 0 | 1 | 🟊 |   `  Engine type:  4 stroke air cooling horizontal E  Production year:  2017： H 2018：J  2019： K 2020：L  Check Number calculated automatically. Possible character including:  **0, 1, 2, 3, 4, 5, 6, 7, 8, 9, X**  Transmission type：Belt drire P  Vehicle type: motorscooter T  Engine displacement: 125CC J  Design NO.: J  WMI： L4H  Manufacturer code： 6  Running number： |