|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| Structure of VIN system

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| 🟊 | L | 4 | H | S | T | E | J | P | ? | H | 6 | 0 | 0 | 0 | 0 | 0 | 1 | 🟊 |

`Engine type: 4 stroke air cooling horizontal EProduction year:2017： H 2018：J2019： K 2020：LCheck Number calculated automatically. Possible character including:**0, 1, 2, 3, 4, 5, 6, 7, 8, 9, X**Transmission type：Belt drire PVehicle type: motorscooter TEngine displacement: 125CC JDesign NO.: SWMI： L4HManufacturer code： 6Running number： |